{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":4,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[null,"6150 Impuls CVT","6165 Impuls CVT","6175 Impuls CVT"]
["Engine"]
["Number of cylinders ",6,6,6]
["Type ","Common Rail Diesel engine with 24 valves, turbocharged and intercooled","Common Rail Diesel engine with 24 valves, turbocharged and intercooled","Common Rail Diesel engine with 24 valves, turbocharged and intercooled"]
["Emission Level ","Stage V","Stage V","Stage V"]
["Capacity (cm³) ",6728,6728,6728]
["Engine Performance"]
["Maximum engine power with Power Management (hp (kW)) ","190 (140)","210 (155)","225 (166)"]
["Maximum engine power (hp (kW)) ","165 (121)","180 (132)","180 (132)"]
["@ engine speed (rpm) ","1800–1900","1800–1900","1800–1900"]
["Rated engine power with Power Management (hp (kW)) ","175 (129)","190 (140)","205 (151)"]
["Rated engine power (hp (kW)) ","150 (110)","165 (121)","180 (132)"]
["Rated engine speed (rpm) ",2200,2200,2200]
["Maximum torque Power Management (Nm @ rpm) ","805 @ 1500","875 @ 1500","940 @ 1500"]
["Maximum torque (Nm @ rpm) ","700 @ 1500","770 @ 1500","770 @ 1500"]
["Torque rise Standard and Power Management (%) ","46 / 44","46 / 44","46 / 44"]
["Fuel tank capacity diesel / urea (litres) ","330 / 48","330 / 48","330 / 48"]
["Standard Transmission"]
["Transmission Type ","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission"]
["Maximum Speed Forward (kp/h) ","40 Eco / 50 Eco","40 Eco / 50 Eco","40 Eco / 50 Eco"]
["Powershuttle ","Standard","Standard","Standard"]
["Creeper ","integrated","integrated","integrated"]
["Optional Transmission 1"]
["Transmission Type ","-","-","-"]
["Maximum Speed Forward (kp/h) ","-","-","-"]
["Powershuttle ","-","-","-"]
["Creeper ","-","-","-"]
["Optional Transmission 2"]
["Transmission Type ","-","-","-"]
["Maximum Speed Forward (km/h) ","-","-","-"]
["Powershuttle ","-","-","-"]
["Creeper ","-","-","-"]
["Power Take Off"]
["PTO Type ","Electro-hydraulic with Auto PTO control available","Electro-hydraulic with Auto PTO control available","Electro-hydraulic with Auto PTO control available"]
["Speed Standard @ rpm ","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893"]
["Speed Optional @ rpm ","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621"]
["Ground drive ","-","-","-"]
["Shaft type ","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)"]
["Front PTO and hitch"]
["Speed Standard @ rpm ","1000 @ 1895","1000 @ 1895","1000 @ 1895"]
["Front hitch lift capacity (kg) ",3568,3568,3568]
["Drive and Steering (Driveline)"]
["2WD ","-","-","-"]
["4WD ","Yes","Yes","Yes"]
["Front axle suspension ","Standard","Standard","Standard"]
["Steering angle (°) ",55,55,55]
["Min.turning radius (m) ",5.45,5.45,5.45]
["Rear axle diff-lock ","Multi disc wet plate with management system","Multi disc wet plate with management system","Multi disc wet plate with management system"]
["Service Brake Type ","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting"]
["ABS Anti-lock braking system ","-","-","-"]
["Hydraulic System"]
["System Type ","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump"]
["Max. pump flow rate Standard / Option (litres) ","147 / 166","147 / 166","147 / 166"]
["System pressure (bar) ",210,210,210]
["Control type ","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control"]
["Max. lift capacity (kg) ",8257,8257,8257]
["OECD lift capacity through range @ 610 mm (kg) ",6616,6616,6616]
["Max. number of rear remotes valves ","5 elec.","5 elec.","5 elec."]
["Max. number of mid mount valves ",3,3,3]
["Remote valve timer control ","0-60 seconds","0-60 seconds","0-60 seconds"]
["Category type ","Cat. III","Cat. III","Cat. III"]
["Slip control ","Standard","Standard","Standard"]