{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":4,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[null,"4100 Multi","4110 Multi","4120 Multi"]
["Engine"]
["Number of cylinders ",4,4,4]
["Type ","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 16 valves, turbocharged and intercooled"]
["Emission Level ","Stage V","Stage V","Stage V"]
["Capacity (cm³) ",3600,3600,3600]
["Engine Performance"]
["Maximum engine power with Power Management (hp (kW)) ","-","-","-"]
["Maximum engine power (hp (kW)) ","-","-","-"]
["@ engine speed (rpm) ","-","-","-"]
["Rated engine power with Power Management (hp (kW)) ","-","-","-"]
["Rated engine power (hp (kW)) ","101 (74)","110 (81)","117 (86)"]
["Rated engine speed (rpm) ",2300,2300,2300]
["Maximum torque Power Management (Nm @ rpm) "," "," "," "]
["Maximum torque (Nm @ rpm) ","450 @ 1300","490 @ 1300","506 @ 1300"]
["Torque rise Standard and Power Management (%) ","47 / -","46 / -","42 / -"]
["Fuel tank capacity diesel / urea (litres) ","145 / 14","145 / 14","145 / 14"]
["Standard Transmission"]
["Transmission Type ","S-Control 4 - 32 x32 automated 4-stage synchromesh transmission","S-Control 4 - 32 x32 automated 4-stage synchromesh transmission","S-Control 4 - 32 x32 automated 4-stage synchromesh transmission"]
["Maximum Speed Forward (kp/h) ",40,40,40]
["Powershuttle ","Standard","Standard","Standard"]
["Creeper ","-","-","-"]
["Optional Transmission 1"]
["Transmission Type ","S-Control 4 with Pack-lock","S-Control 4 with Pack-lock","S-Control 4 with Pack-lock"]
["Maximum Speed Forward (kp/h) ",40,40,40]
["Powershuttle ","Standard","Standard","Standard"]
["Creeper ","-","-","-"]
["Optional Transmission 2"]
["Transmission Type ","-","-","-"]
["Maximum Speed Forward (km/h) ","-","-","-"]
["Powershuttle ","-","-","-"]
["Creeper ","-","-","-"]
["Power Take Off"]
["PTO Type ","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement"]
["Speed Standard @ rpm ","540/540E/1000/1000E @ 1805 / 1542 / 1880 / 1606","540/540E/1000/1000E @ 1805 / 1542 / 1880 / 1606","540/540E/1000/1000E @ 1805 / 1542 / 1880 / 1606"]
["Speed Optional @ rpm ","-","-","-"]
["Ground drive ","Option","Option","Option"]
["Shaft type ","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)"]
["Front PTO and hitch"]
["Speed Standard @ rpm ","1000 @ 1920","1000 @ 1920","1000 @ 1920"]
["Front hitch lift capacity (kg) ",1985,1985,1985]
["Drive and Steering (Driveline)"]
["2WD ","-","-","-"]
["4WD ","Yes","Yes","Yes"]
["Front axle suspension ","Option","Option","Option"]
["Steering angle (°) ",55,55,55]
["Min.turning radius (m) ",4.28,4.28,4.28]
["Rear axle diff-lock ","Electro-hydraulic","Electro-hydraulic","Electro-hydraulic"]
["Service Brake Type ","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting"]
["ABS Anti-lock braking system ","-","-","-"]
["Hydraulic System"]
["System Type ","Pressure flow compensated pump","Pressure flow compensated pump","Pressure flow compensated pump"]
["Max. pump flow rate Standard / Option (litres) ","80 / 100","80 / 100","80 / 100"]
["System pressure (bar) ","170 / 200","170 / 200","170 / 200"]
["Control type ","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control"]
["Max. lift capacity (kg) ",5550,5550,5550]
["OECD lift capacity through range @ 610 mm (kg) ",4700,4700,4700]
["Max. number of rear remotes valves ",4,4,4]
["Max. number of mid mount valves ",2,2,2]
["Remote valve timer control ","0–30 seconds","0–30 seconds","0–30 seconds"]
["Category type ","Cat. II / III N","Cat. II / III N","Cat. II / III N"]
["Slip control ","Option","Option","Option"]