{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[null,"4115 Profi CVT","4125 Profi CVT","4135 Profi CVT","4145 Profi CVT","6150 Profi CVT"]
["Engine"]
["Number of cylinders ",4,4,4,4,6]
["Type ","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 16 valves, turbocharged and intercooled","Common Rail Diesel engine with 24 valves, turbocharged and intercooled"]
["Emission Level ","Stage V  Stage V","Stage V  Stage V","Stage V  Stage V","Stage V  Stage V","Stage V  Stage V  Stage V"]
["Capacity (cm³) ",4485,4485,4485,4485,6728]
["Engine Performance"]
["Maximum engine power with Power Management (hp (kW)) ","145 (107)","155 (114)","169 (124)","175 (129)","175 (129)"]
["Maximum engine power (hp (kW)) ","125 (92)","135 (99)","145 (107)","155 (114)","158 (116)"]
["@ engine speed (rpm) ","1800–1900","1800–1900","1800–1900","1800–1900","1800–1900"]
["Rated engine power with Power Management (hp (kW)) ","131 (96)","140 (103)","155 (114)","160 (118)","165 (121)"]
["Rated engine power (hp (kW)) ","116 (85)","125 (92)","135 (99)","145 (107)","150 (110)"]
["Rated engine speed (rpm) ",2200,2200,2200,2200,2200]
["Maximum torque Power Management (Nm @ rpm) ","590 @ 1500","637 @ 1500","700 @ 1500","700 @ 1500","740 @ 1500"]
["Maximum torque (Nm @ rpm) ","528 @ 1500","560 @ 1500","605 @ 1500","650 @ 1500","650 @ 1500"]
["Torque rise Standard and Power Management (%) ","41 / 42","40 / 43","40 / 42","40 / 37","40 / 40"]
["Fuel tank capacity diesel / urea (litres) ","210 (250) / 39.5","210 (250) / 39.5","210 (250) / 39.5","210 (250) / 39.5","210 (250) / 39.5"]
["Standard Transmission"]
["Transmission Type ","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission","S-Control CVT - continuously variable transmission"]
["Maximum Speed Forward (kp/h) ","50 or 40 Eco","50 or 40 Eco","50 or 40 Eco","50 or 40 Eco","50 or 40 Eco"]
["Powershuttle ","Standard","Standard","Standard","Standard","Standard"]
["Creeper ","integrated","integrated","integrated","integrated","integrated"]
["Optional Transmission 1"]
["Transmission Type ","-","-","-","-",0]
["Maximum Speed Forward (kp/h) ","-","-","-","-",0]
["Powershuttle ","-","-","-","-",0]
["Creeper ","-","-","-","-",0]
["Optional Transmission 2"]
["Transmission Type ","-","-","-","-","-"]
["Maximum Speed Forward (km/h) ","-","-","-","-","-"]
["Powershuttle ","-","-","-","-","-"]
["Creeper ","-","-","-","-","-"]
["Power Take Off"]
["PTO Type ","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement","Shiftable with progressive electro-hydraulic engagement"]
["Speed Standard @ rpm ","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893","540 / 540E / 1000 @ 1969 / 1546 / 1893"]
["Speed Optional @ rpm ","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621","540E / 1000 / 1000E @ 1592 / 1893 / 1621"]
["Ground drive ","Option","Option","Option","Option","Option"]
["Shaft type ","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)"]
["Front PTO and hitch"]
["Speed Standard @ rpm ","1000 @ 1895","1000 @ 1895","1000 @ 1895","1000 @ 1895","1000 @ 1895"]
["Front hitch lift capacity (kg) ",3100,3100,3100,3100,3100]
["Drive and Steering (Driveline)"]
["2WD ","-","-","-","-","-"]
["4WD ","Yes","Yes","Yes","Yes","Yes"]
["Front axle suspension ","Option","Option","Option","Option","Option"]
["Steering angle (°) ",55,55,55,55,55]
["Min.turning radius (m) ",4.6,4.6,4.6,4.6,4.6]
["Rear axle diff-lock ","Multi disc wet plate with management system","Multi disc wet plate with management system","Multi disc wet plate with management system","Multi disc wet plate with management system","Multi disc wet plate with management system"]
["Service Brake Type ","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting"]
["ABS Anti-lock braking system ","-","-","-","-","-"]
["Hydraulic System"]
["System Type ","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump","Variable displacement, pressure flow compensated pump"]
["Max. pump flow rate Standard / Option (litres) ","150 / -","150 / -","150 / -","150 / -","150 / -"]
["System pressure (bar) ","210 / -","210 / -","210 / -","210 / -","210 / -"]
["Control type ","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control","Electronic Hitch Control (EHC) with hitch ride control"]
["Max. lift capacity (kg) ",7864,7864,7864,7864,7864]
["OECD lift capacity through range @ 610 mm (kg) ",6796,6796,6796,6796,6796]
["Max. number of rear remotes valves ","4 elec.","4 elec.","4 elec.","4 elec.","4 elec."]
["Max. number of mid mount valves ",3,3,3,3,3]
["Remote valve timer control ","0–30 seconds","0–30 seconds","0–30 seconds","0–30 seconds","0–30 seconds"]
["Category type ","Cat. II / III","Cat. II / III","Cat. II / III","Cat. II / III","Cat. II / III"]
["Slip control ","Option","Option","Option","Option","Option"]