{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[null,"4080 Kompakt","4090 Kompakt","4100 Kompakt","4110 Kompakt","4120 Kompakt"]
["Engine"]
["Number of cylinders ",4,4,4,4,4]
["Type ","Common-rail diesel engine, turbocharged and intercooled","Common-rail diesel engine, turbocharged and intercooled","Common-rail diesel engine, turbocharged and intercooled","Common-rail diesel engine, turbocharged and intercooled","Common-rail diesel engine, turbocharged and intercooled"]
["Emission Level ","Stage V","Stage V","Stage V","Stage V","Stage V"]
["Capacity (cm³) ",3600,3600,3600,3600,3600]
["Engine Performance"]
["Maximum engine power with Power Management (hp (kW)) ","-","-","-","-","-"]
["Maximum engine power (hp (kW)) ","-","-","-","-","-"]
["@ engine speed (rpm) ","-","-","-","-","-"]
["Rated engine power with Power Management (hp (kW)) ","-","-","-","-","-"]
["Rated engine power (hp (kW)) ","80 (59)","90 (66)","100 (74)","110 (81)","120 (86)"]
["Rated engine speed (rpm) ",2300,2300,2300,2300,2300]
["Maximum torque Power Management (Nm @ rpm) ","-","-","-","-","-"]
["Maximum torque (Nm @ rpm) ","330 @ 1300","380 @ 1300","450 @ 1300","490 @ 1300","506 @ 1300"]
["Torque rise Standard and Power Management (%) ","41,7 / -","45,7 / -","46,5 / -","38,7 / -","34,7 / -"]
["Fuel tank capacity diesel / urea (litres) ","128.8 / 9.6","128.8 / 9.6","128.8 / 9.6","128.8 / 9.6","128.8 / 9.6"]
["Standard Transmission"]
["Transmission Type ","S-Control M - 12 x 12 Synchroshift with mechanical shuttle","S-Control M - 12 x 12 Synchroshift with mechanical shuttle","S-Control M - 12 x 12 Synchroshift with mechanical shuttle","S-Control M - 12 x 12 Synchroshift with mechanical shuttle","S-Control M - 12 x 12 Synchroshift with mechanical shuttle"]
["Maximum Speed Forward (kp/h) ",40,40,40,40,40]
["Powershuttle ","Option","Option","Option","Option","Option"]
["Creeper ","Option","Option","Option","Option","Option"]
["Optional Transmission 1"]
["Transmission Type ","S-Control M - 12 x 12 Synchroshift with Powershuttle","S-Control M - 12 x 12 Synchroshift with Powershuttle","S-Control M - 12 x 12 Synchroshift with Powershuttle","S-Control M - 12 x 12 Synchroshift with Powershuttle","S-Control M - 12 x 12 Synchroshift with Powershuttle"]
["Maximum Speed Forward (kp/h) ",40,40,40,40,40]
["Powershuttle ","Standard","Standard","Standard","Standard","Standard"]
["Creeper ","Option","Option","Option","Option","Option"]
["Optional Transmission 2"]
["Transmission Type ","S-Control 2 - 24x24 gears, 2-speed Powershift","S-Control 2 - 24x24 gears, 2-speed Powershift","S-Control 2 - 24x24 gears, 2-speed Powershift","S-Control 2 - 24x24 gears, 2-speed Powershift","S-Control 2 - 24x24 gears, 2-speed Powershift"]
["Maximum Speed Forward (km/h) ",40,40,40,40,40]
["Powershuttle ","Standard","Standard","Standard","Standard","Standard"]
["Creeper ","Option","Option","Option","Option","Option"]
["Power Take Off"]
["PTO Type ","Servo assisted / electro-hydraulic engagement optional","Servo assisted / electro-hydraulic engagement optional","Servo assisted / electro-hydraulic engagement optional","Servo assisted / electro-hydraulic engagement optional","Servo assisted / electro-hydraulic engagement optional"]
["Speed Standard @ rpm ","540 / 540E / 1000 @ 1,938 / 1,535 / 1,926","540 / 540E / 1000 @ 1,938 / 1,535 / 1,926","540 / 540E / 1000 @ 1,938 / 1,535 / 1,926","540 / 540E / 1000 @ 1,938 / 1,535 / 1,926","540 / 540E / 1000 @ 1,938 / 1,535 / 1,926"]
["Speed Optional @ rpm ","-","-","-","-","-"]
["Ground drive ","Option","Option","Option","Option","Option"]
["Shaft type ","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)","1 3/8\" 21 splines (1 3/8\" 6 splines)"]
["Front PTO and hitch"]
["Speed Standard @ rpm ","1000 @ 1920","1000 @ 1920","1000 @ 1920","1000 @ 1920","1000 @ 1920"]
["Front hitch lift capacity (kg) ",1670,1670,1670,1670,1670]
["Drive and Steering (Driveline)"]
["2WD ","-","-","-","-","-"]
["4WD ","Yes","Yes","Yes","Yes","Yes"]
["Front axle suspension ","-","-","-","-","-"]
["Steering angle (°) ",55,55,55,55,55]
["Min.turning radius (m) ",4.23,4.23,4.23,4.23,4.23]
["Rear axle diff-lock ","Electro-hydraulic","Electro-hydraulic","Electro-hydraulic","Electro-hydraulic","Electro-hydraulic"]
["Service Brake Type ","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting","Hydraulically operated multiple wet disc brake, self adjusting"]
["ABS Anti-lock braking system ","-","-","-","-","-"]
["Hydraulic System"]
["System Type ","Pressure flow compensated pump","Pressure flow compensated pump","Pressure flow compensated pump","Pressure flow compensated pump","Pressure flow compensated pump"]
["Max. pump flow rate Standard / Option (litres) ","64 / -","64 / -","64 / -","64 / -","64 / -"]
["System pressure (bar) "," "," "," "," "," "]
["Control type ","Electronical Hitch Control (EHC)","Electronical Hitch Control (EHC)","Electronical Hitch Control (EHC)","Electronical Hitch Control (EHC)","Electronical Hitch Control (EHC)"]
["Max. lift capacity (kg) ",4400,4400,4400,4400,4400]
["OECD lift capacity through range @ 610 mm (kg) ",3350,3350,3350,3350,3350]
["Max. number of rear remotes valves ",3,3,3,3,3]
["Max. number of mid mount valves ",2,2,2,2,2]
["Remote valve timer control ","-","-","-","-","-"]
["Category type ","Cat II","Cat II","Cat II","Cat II","Cat II"]
["Slip control ","-","-","-","-","-"]